SECTION 129300

SITE FURNISHINGS

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**NOTE TO SPECIFIER**

*Use this Specification Section for Mail Processing Facilities.*

***This is a Type 1 Specification with completely editable text; therefore, any portion of the text can be modified by the A/E preparing the Solicitation Package to suit the project.***

*For Design/Build projects, do not delete the Notes to Specifier in this Section so that they may be available to Design/Build entity when preparing the Construction Documents.*

*For the Design/Build entity, this specification is intended as a guide for the Architect/Engineer preparing the Construction Documents.*

*The MPF specifications may also be used for Design/Bid/Build projects. In either case, it is the responsibility of the design professional to edit the Specifications Sections as appropriate for the project.*

*Text shown in brackets must be modified as needed for project specific requirements.* *See the “Using the USPS Guide Specifications” document in Folder C for more information.*

*The last date that USPS revised this standard specification section occurs in two places, at the end of this section and in the Table of Contents. If the date in this section matches the date in the Table of Contents, then you are using the latest version. Do not delete or revise the “last revised” date at the end of the section during the development of the Project Manual.*

*The footer in this section should be edited to replace the text, “USPS MPF SPECIFICATION” with the project name, and the blank date in the center should be replaced with the submission date, for interim design reviews, or the issue date of the completed Project Manual.*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

1. GENERAL
   1. SUMMARY
      1. Section Includes:
         1. Bicycle racks.
         2. Parking blocks.
         3. Landscape decorative bollards.
      2. Related Documents: The Contract Documents, as defined in Section 011000- Summary of Work, apply to the Work of this Section. Additional requirements and information necessary to complete the Work of this Section may be found in other Documents.
   2. SUBMITTALS
      1. Section 013300 - Submittal Procedures: Procedures for submittals.
         1. Product Data: Indicate materials, construction, configuration, dimensions, and finishes.
         2. Assurance/Control Submittals:
            1. Certificates: Manufacturer's certificate that Products meet or exceed specified requirements.
   3. DELIVERY, STORAGE, AND HANDLING
      1. Section 016000 - Product Requirements: Transport, handle, store, and protect Products.
2. PRODUCTS

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**NOTE TO SPECIFIER**

Bicycle Rack and Parking Blocks are included below. If other Site Furnishings are required, specify them in this Section. Verify manufacturer information, products, and availability at time of Project Manual preparation for Project.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

* 1. BICYCLE RACK
     1. Manufacturer: Subject to compliance with project requirements, manufacturers offering products which may be incorporated in the Work include the following:
        1. Brandir International, New York, NY (212) 505-6500.
        2. Huntco Supply, LLC, Portland, OR (800) 547-5909.
        3. Trilary, Incorporated, Middleton, WI (800) 448-7931.
     2. Section 016000 - Product Requirements: Product options and substitutions. Substitutions: Permitted.
     3. Model:
        1. Brandir: #RB-051G.
        2. Huntco: #BR 5 SF-G.
        3. Trilary: #H36-5-SF-G.
     4. Ribbon Rack: 5 bicycle capacity, ground anchored.
        1. ASTM A 53, Schedule 40 galvanized pipe with 2.375 inch O.D. x 0.154 inch thick wall, hot-dipped galvanized after fabrication.
  2. PARKING BLOCKS
     1. Manufacturers: Subject to compliance with project requirements, manufacturers offering products which may be incorporated in the Work include the following:
        1. Amazing Recycled Products, Denver, CO (800) 241-2174.
        2. American Recreational Products, Ronkonkoma, NY (800) 663-4096.
        3. The Parking Block Store, Sherwood, MD (800) 683-9963.
        4. Phoenix Recycled Plastics Corporation, Ambler, PA (215) 653-0300.
     2. Section 016000 - Product Requirements: Product options and substitutions. Substitutions: Permitted.
     3. Model:
        1. Amazing: #ARP8150.
        2. American: #PB4-6
        3. Parking Block Store: Saver Block.
        4. Phoenix: Paving Maintenance Products (stops).
     4. Design: Solid block, 6 feet long by 4 inches high. Manufactured from 100% recycled plastic. Anchoring as recommended by manufacturer.
     5. Color: Homogenous. Gray.
  3. LANDSCAPE BOLLARDS
     1. Manufacturer: Subject to compliance with project requirements, manufacturers offering products which may be incorporated in the work include the following:
        1. Wausau Tile, Inc., Wausau, Wisconsin, 800-388-8728.
     2. Section 016000 Product Requirements: Product options and substitutions: Permitted.
     3. Model
        1. Wausau #TF6066: Reinforced concrete circle 14x16x39, 600 lbs., standard Weatherstone colors.

1. EXECUTION
   1. EXAMINATION
      1. Section 017300 - Execution: Verification of existing conditions before starting work.
      2. Verification of Conditions: Verify that field measurements, surfaces, substrates, and conditions are as required, and ready to receive Work.
      3. Report in writing to Contracting Officer prevailing conditions that will adversely affect satisfactory execution of the Work of this Section. Do not proceed with Work until unsatisfactory conditions have been corrected.
      4. By beginning Work, Contractor accepts conditions and assumes responsibility for correcting unsuitable conditions encountered at no additional cost to USPS.
   2. INSTALLATION
      1. Install in accordance with manufacturer's published instructions at locations indicated on Drawings.

END OF SECTION

USPS MPF Specification Last Revised: 10/1/2022