Yonkers Fire Station 14

Supplemental Specification

1. Per Note 3 on Drawing S-100, contractor is to assume that the soil beneath the 8” of stone under the slab is contaminated. This depth could vary by area within the slab. For bidding purposes, the contractor shall assume the depth of excavation is 20” for the slab from top of existing slab to bottom of excavation. Additionally, the contractor’s bid pricing shall include the soil removals for the pile caps, piles, and exterior concrete apron.
2. The basis of design for the project’s replacement drains is JR Smith #2624 galvanized. Provide this or approved equal.
3. The contractor shall refer to and comply with Technical Specification Section 026100 - Removal and Disposal of Contaminated Soils, which is provided with this supplement.